Thank you to our hosts for providing the networking at the conference location!

At Stanford, wireless access will be provided using two special SSIDs, in addition to eduroam.  The two SSIDs will be J-Techs and JT-v6, and will be available in public areas around campus.  The J-Techs and JT-v6 SSIDs are using a WPA2 pre shared key.  The password for these networks is **Summer2012**.  Below are some technical details for those that are interested

The wired IP network for the Laptop Bar uses 171.66.6.128/26 and 2607:F6D0:CED:5DB::0/64

In the meeting building, LKSC, there will be a special instance of the

eduroam SSID being provided.  Which will have public IPv4 addresses in

the block 171.66.12.0/22 and IPv6 prefix 2607:F6D0:CED:5DA::0/64.

For eduroam around the rest of campus, it will receive IPv6 from the

address block 2607:F6D0:CED:500::0/56 and be doing IPv4 NAT/PAT into

the range 68.65.174.0/24

The J-Techs SSID uses 171.66.8.0/22 and 2607:F6D0:CED:5D9::0/64

The JT-v6 SSID uses 2607:F6D0:CED:5D8::0/64.  On that SSID, we are

also attempting to run stateless DHCPv6 to deliver the IPv6 DNS

address, which is 2607:f6d0:ced:5d8:171:67:248:69

Due to technical difficulties we will not be able to source a multicast stream from the meeting venue as a netcast viewing option.